
(constraints
	(version "5.0.0")
	(objectType ORPHANS
		(object_count 0))
	(objectType PARALLEL_RULE
		(object_count 0))
	(objectType SCHEME_RULE_LAYER
		(object_count 12)
		(co "(Master)" "Scheme"
			(cv UVIA_SAME_NET "FALSE")
			(cv UVIA_C2C "FALSE")
			(co "(Master)/(Default Rule)" "ClearRule" "(Default Rule)"
				(cv UVIA_SAME_NET "FALSE")
				(cv UVIA_C2C "FALSE")
				(o "(Master)/(Default Rule)/SIGNAL_1" "Layer" "SIGNAL_1"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_TRACE "10")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150")
					(cv MASK_TO_RESISTOR "10"))
				(o "(Master)/(Default Rule)/PLANE_2" "Layer" "PLANE_2"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_TRACE "10")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150")
					(cv MASK_TO_RESISTOR "10"))
				(o "(Master)/(Default Rule)/PLANE_3" "Layer" "PLANE_3"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_TRACE "10")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150")
					(cv MASK_TO_RESISTOR "10"))
				(o "(Master)/(Default Rule)/SIGNAL_4" "Layer" "SIGNAL_4"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_TRACE "10")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150")
					(cv MASK_TO_RESISTOR "10"))))
		(co "(Minimum)" "Scheme"
			(cv UVIA_SAME_NET "FALSE")
			(cv UVIA_C2C "FALSE")
			(co "(Minimum)/(Default Rule)" "ClearRule" "(Default Rule)"
				(cv UVIA_SAME_NET "FALSE")
				(cv SRLNAME "(Default Rule)")
				(cv UVIA_C2C "FALSE")
				(o "(Minimum)/(Default Rule)/SIGNAL_1" "Layer" "SIGNAL_1"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv RESISTOR_TO_TRACE "10")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv SRLNAME "SIGNAL_1")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv MASK_TO_RESISTOR "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150"))
				(o "(Minimum)/(Default Rule)/PLANE_2" "Layer" "PLANE_2"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv RESISTOR_TO_TRACE "10")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv SRLNAME "PLANE_2")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv MASK_TO_RESISTOR "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150"))
				(o "(Minimum)/(Default Rule)/PLANE_3" "Layer" "PLANE_3"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv RESISTOR_TO_TRACE "10")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv SRLNAME "PLANE_3")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv MASK_TO_RESISTOR "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150"))
				(o "(Minimum)/(Default Rule)/SIGNAL_4" "Layer" "SIGNAL_4"
					(cv TRACE_TO_PLANE "7.87401574803150")
					(cv TRACE_TO_PAD "7.87401574803150")
					(cv RESISTOR_TO_RESISTOR "10")
					(cv PAD_TO_VIA "7.87401574803150")
					(cv PLANE_TO_PLANE "10")
					(cv VIA_TO_VIA "7.87401574803150")
					(cv PAD_TO_PLANE "7.87401574803150")
					(cv RESISTOR_TO_VIA "10")
					(cv PAD_TO_PAD "7.87401574803150")
					(cv TRACE_TO_TRACE "7.87401574803150")
					(cv MASK_TO_VIA "10")
					(cv MASK_TO_TRACE "10")
					(cv VIA_TO_PLANE "7.87401574803150")
					(cv UVIA_SAME_NET "FALSE")
					(cv RESISTOR_TO_TRACE "10")
					(cv SMDPAD_TO_VIA "7.87401574803150")
					(cv RESISTOR_TO_PAD "10")
					(cv TRACE_TO_VIA "7.87401574803150")
					(cv SRLNAME "SIGNAL_4")
					(cv UVIA_C2C "FALSE")
					(cv MASK_TO_PAD "10")
					(cv MASK_TO_RESISTOR "10")
					(cv SMDPAD_TO_TRACE "7.87401574803150")))))
	(objectType PART
		(object_count 277)
		(co "C-0402" "Part"
			(cv QUANTITY "25")
			(o "C-0402/1" "PartPin" "1")
			(o "C-0402/2" "PartPin" "2")
			(co "C1" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "15N")
				(o "C1-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C1-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C2" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "10N")
				(o "C2-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C2-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C3" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C3-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C3-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C4" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C4-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C4-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C5" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C5-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C5-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C6" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C6-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C6-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C7" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C7-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C7-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C8" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C8-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C8-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C9" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "15P")
				(o "C9-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C9-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C12" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C12-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C12-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C13" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C13-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C13-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C14" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C14-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C14-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C15" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C15-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C15-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C16" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C16-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C16-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C18" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C18-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C18-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C19" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "1U")
				(o "C19-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C19-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C20" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "1U")
				(o "C20-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C20-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C21" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "1U")
				(o "C21-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C21-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C22" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C22-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C22-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C23" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.22U")
				(o "C23-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C23-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C24" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "1N")
				(o "C24-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C24-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C25" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C25-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C25-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C26" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C26-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C26-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C27" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C27-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C27-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "C28" "Comp"
				(cv DEVICE "C-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "0.1U")
				(o "C28-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C28-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "C-TANTAL_CASE_A" "Part"
			(cv QUANTITY "1")
			(o "C-TANTAL_CASE_A/1" "PartPin" "1")
			(o "C-TANTAL_CASE_A/2" "PartPin" "2")
			(co "C17" "Comp"
				(cv DEVICE "C-TANTAL_CASE_A")
				(cv PART_TYPE "Other")
				(cv VALUE "10U")
				(o "C17-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "C17-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "TP" "Part"
			(cv QUANTITY "4")
			(o "TP/1" "PartPin" "1")
			(co "P1" "Comp"
				(cv DEVICE "TP")
				(cv PART_TYPE "Other")
				(o "P1-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "P2" "Comp"
				(cv DEVICE "TP")
				(cv PART_TYPE "Other")
				(o "P2-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "P3" "Comp"
				(cv DEVICE "TP")
				(cv PART_TYPE "Other")
				(o "P3-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "P4" "Comp"
				(cv DEVICE "TP")
				(cv PART_TYPE "Other")
				(o "P4-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "R-0402" "Part"
			(cv QUANTITY "13")
			(o "R-0402/1" "PartPin" "1")
			(o "R-0402/2" "PartPin" "2")
			(co "R1" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "50K")
				(o "R1-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R1-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R2" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "50K")
				(o "R2-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R2-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R3" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "5K")
				(o "R3-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R3-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R4" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "30K")
				(o "R4-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R4-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R8" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "3K")
				(o "R8-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R8-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R9" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "5K")
				(o "R9-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R9-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R11" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "36K")
				(o "R11-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R11-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R12" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "33K")
				(o "R12-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R12-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R13" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "15K")
				(o "R13-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R13-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R14" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "47")
				(o "R14-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R14-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R15" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "33K")
				(o "R15-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R15-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R16" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "16K")
				(o "R16-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R16-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "R17" "Comp"
				(cv DEVICE "R-0402")
				(cv PART_TYPE "Other")
				(cv VALUE "16K")
				(o "R17-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "R17-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "ADG819BRM" "Part"
			(cv QUANTITY "3")
			(o "ADG819BRM/1" "PartPin" "1")
			(o "ADG819BRM/2" "PartPin" "2")
			(o "ADG819BRM/3" "PartPin" "3")
			(o "ADG819BRM/4" "PartPin" "4")
			(o "ADG819BRM/5" "PartPin" "5")
			(o "ADG819BRM/6" "PartPin" "6")
			(o "ADG819BRM/7" "PartPin" "7")
			(o "ADG819BRM/8" "PartPin" "8")
			(co "U2" "Comp"
				(cv DEVICE "ADG819BRM")
				(cv PART_TYPE "Other")
				(o "U2-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "D.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U2-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "S1.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U2-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U2-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "VDD.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U2-5" "CompPin"
					(cv PIN_GROUP "L")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U2-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "IN.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U2-7" "CompPin"
					(cv PIN_GROUP "L")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U2-8" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "S2.8")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "U3" "Comp"
				(cv DEVICE "ADG819BRM")
				(cv PART_TYPE "Other")
				(o "U3-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "D.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U3-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "S1.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U3-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U3-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "VDD.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U3-5" "CompPin"
					(cv PIN_GROUP "L")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U3-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "IN.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U3-7" "CompPin"
					(cv PIN_GROUP "L")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U3-8" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "S2.8")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "U4" "Comp"
				(cv DEVICE "ADG819BRM")
				(cv PART_TYPE "Other")
				(o "U4-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "D.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U4-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "S1.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U4-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U4-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "VDD.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U4-5" "CompPin"
					(cv PIN_GROUP "L")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U4-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "IN.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U4-7" "CompPin"
					(cv PIN_GROUP "L")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U4-8" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "S2.8")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "AD822ARM" "Part"
			(cv QUANTITY "2")
			(o "AD822ARM/1" "PartPin" "1")
			(o "AD822ARM/2" "PartPin" "2")
			(o "AD822ARM/3" "PartPin" "3")
			(o "AD822ARM/4" "PartPin" "4")
			(o "AD822ARM/5" "PartPin" "5")
			(o "AD822ARM/6" "PartPin" "6")
			(o "AD822ARM/7" "PartPin" "7")
			(o "AD822ARM/8" "PartPin" "8")
			(co "U5" "Comp"
				(cv DEVICE "AD822ARM")
				(cv PART_TYPE "Other")
				(o "U5-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "OUT.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-IN.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+IN.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-V.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+IN.5")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-IN.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-7" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "OUT.7")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U5-8" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+V.8")
					(cv ASSIGN_PIN_GROUP "S")))
			(co "U13" "Comp"
				(cv DEVICE "AD822ARM")
				(cv PART_TYPE "Other")
				(o "U13-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "OUT.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-IN.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+IN.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-V.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+IN.5")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-IN.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-7" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "OUT.7")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U13-8" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+V.8")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "AD8605ART" "Part"
			(cv QUANTITY "1")
			(o "AD8605ART/1" "PartPin" "1")
			(o "AD8605ART/2" "PartPin" "2")
			(o "AD8605ART/3" "PartPin" "3")
			(o "AD8605ART/4" "PartPin" "4")
			(o "AD8605ART/5" "PartPin" "5")
			(co "U6" "Comp"
				(cv DEVICE "AD8605ART")
				(cv PART_TYPE "Other")
				(o "U6-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "OUT")
					(cv REALPINDATA "OUT.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U6-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "V-.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U6-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "+IN.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U6-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "-IN.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U6-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "V+.5")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "LTC1799CS5" "Part"
			(cv QUANTITY "1")
			(o "LTC1799CS5/1" "PartPin" "1")
			(o "LTC1799CS5/2" "PartPin" "2")
			(o "LTC1799CS5/3" "PartPin" "3")
			(o "LTC1799CS5/4" "PartPin" "4")
			(o "LTC1799CS5/5" "PartPin" "5")
			(co "U8" "Comp"
				(cv DEVICE "LTC1799CS5")
				(cv PART_TYPE "Other")
				(o "U8-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "V+.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U8-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U8-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "SET.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U8-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "DIV.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U8-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "OUT.5")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "ADP3335ARM" "Part"
			(cv QUANTITY "1")
			(o "ADP3335ARM/1" "PartPin" "1")
			(o "ADP3335ARM/2" "PartPin" "2")
			(o "ADP3335ARM/3" "PartPin" "3")
			(o "ADP3335ARM/4" "PartPin" "4")
			(o "ADP3335ARM/5" "PartPin" "5")
			(o "ADP3335ARM/6" "PartPin" "6")
			(o "ADP3335ARM/7" "PartPin" "7")
			(o "ADP3335ARM/8" "PartPin" "8")
			(co "U9" "Comp"
				(cv DEVICE "ADP3335ARM")
				(cv PART_TYPE "Other")
				(cv VALUE "ADP3335")
				(o "U9-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "OUT")
					(cv REALPINDATA "OUT1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U9-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "OUT")
					(cv REALPINDATA "OUT2.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U9-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "OUT")
					(cv REALPINDATA "OUT3.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U9-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U9-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "NR.5")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U9-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "~SD.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U9-7" "CompPin"
					(cv PIN_GROUP "L")
					(cv PINTYPE "IN")
					(cv REALPINDATA "IN2.7")
					(cv ASSIGN_PIN_GROUP "L"))
				(o "U9-8" "CompPin"
					(cv PIN_GROUP "L")
					(cv PINTYPE "IN")
					(cv REALPINDATA "IN1.8")
					(cv ASSIGN_PIN_GROUP "L"))))
		(co "ADR03AKS" "Part"
			(cv QUANTITY "1")
			(o "ADR03AKS/1" "PartPin" "1")
			(o "ADR03AKS/2" "PartPin" "2")
			(o "ADR03AKS/3" "PartPin" "3")
			(o "ADR03AKS/4" "PartPin" "4")
			(o "ADR03AKS/5" "PartPin" "5")
			(co "U10" "Comp"
				(cv DEVICE "ADR03AKS")
				(cv PART_TYPE "Other")
				(cv VALUE "ADR03")
				(o "U10-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "TEMP.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U10-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U10-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "VIN.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U10-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "VOUT.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U10-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "TRIM.5")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "ARK_SIMPLE" "Part"
			(cv QUANTITY "1")
			(o "ARK_SIMPLE/1" "PartPin" "1")
			(o "ARK_SIMPLE/1.2" "PartPin" "1.2")
			(o "ARK_SIMPLE/1.5" "PartPin" "1.5")
			(o "ARK_SIMPLE/2.3" "PartPin" "2.3")
			(o "ARK_SIMPLE/2.6" "PartPin" "2.6")
			(o "ARK_SIMPLE/4" "PartPin" "4")
			(o "ARK_SIMPLE/7" "PartPin" "7")
			(co "U11" "Comp"
				(cv DEVICE "ARK_SIMPLE")
				(cv PART_TYPE "Other")
				(cv VALUE "UNKNOWN")
				(o "U11-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U11-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "C1.1.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U11-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "C1.2.3")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U11-4" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "CM.4")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U11-5" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "C2.1.5")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U11-6" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "C2.2.6")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U11-7" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "GND2.7")
					(cv ASSIGN_PIN_GROUP "S"))))
		(co "R-VAR-22AR5KLFTR" "Part"
			(cv QUANTITY "1")
			(o "R-VAR-22AR5KLFTR/1" "PartPin" "1")
			(o "R-VAR-22AR5KLFTR/2" "PartPin" "2")
			(o "R-VAR-22AR5KLFTR/3" "PartPin" "3")
			(co "U12" "Comp"
				(cv DEVICE "R-VAR-22AR5KLFTR")
				(cv PART_TYPE "Other")
				(o "U12-1" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "1.1")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U12-2" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "2.2")
					(cv ASSIGN_PIN_GROUP "S"))
				(o "U12-3" "CompPin"
					(cv PIN_GROUP "S")
					(cv PINTYPE "BI")
					(cv REALPINDATA "3.3")
					(cv ASSIGN_PIN_GROUP "S")))))
	(objectType PKGTYPE_PKGTYPE_RULE
		(object_count 0))
	(objectType COMPLEX_FORMULA
		(object_count 0))
	(objectType ENET
		(object_count 126)
		(co "(All)" "Rule" "(All)"
			(cv ORDER_TYPE "MST")
			(cv POWER_NET "FALSE")
			(cv ECLASS "(All)")
			(cv STUB_LENGTH "300")
			(cv JUMPERS_ALLOWED "Yes")
			(cv BUS "FALSE")
			(cv DELAY_TYPE "Length")
			(cv SIM_DELAY_TYPE "Both")
			(cv ANALOG "FALSE")
			(cv OLDELECNET "FALSE")
			(co "$1N7" "ElecNet"
				(cv PIN_COUNT "3")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N7" "Net" "$1N7"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N7")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "61441")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "U4-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U11-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U11-3" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N9" "ElecNet"
				(cv PIN_COUNT "3")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N9" "Net" "$1N9"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N9")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "73729")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "U3-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U11-5" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U11-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N60" "ElecNet"
				(cv PIN_COUNT "5")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N60" "Net" "$1N60"
					(cv PIN_COUNT "5")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N60")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "53249")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C3-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R3-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U3-8" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U4-8" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U5-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N68" "ElecNet"
				(cv PIN_COUNT "3")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N68" "Net" "$1N68"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N68")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "57345")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C3-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U2-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U5-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N85" "ElecNet"
				(cv PIN_COUNT "4")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N85" "Net" "$1N85"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N85")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "65537")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "R3-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R4-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R8-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U6-4" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N88" "ElecNet"
				(cv PIN_COUNT "3")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N88" "Net" "$1N88"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N88")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "69633")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "R4-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R17-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U6-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N97" "ElecNet"
				(cv PIN_COUNT "3")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N97" "Net" "$1N97"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N97")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "77825")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "R8-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R9-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U12-3" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N156" "ElecNet"
				(cv PIN_COUNT "2")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N156" "Net" "$1N156"
					(cv PIN_COUNT "2")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N156")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "4097")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "R11-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U8-3" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N237" "ElecNet"
				(cv PIN_COUNT "4")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N237" "Net" "$1N237"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N237")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "8193")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C19-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R13-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R16-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U13-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N239" "ElecNet"
				(cv PIN_COUNT "4")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N239" "Net" "$1N239"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N239")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "16385")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C19-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R16-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R17-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U13-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "$1N271" "ElecNet"
				(cv PIN_COUNT "2")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N271" "Net" "$1N271"
					(cv PIN_COUNT "2")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N271")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "32769")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C24-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U9-5" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "GEN" "ElecNet"
				(cv PIN_COUNT "4")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "GEN" "Net" "GEN"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "GEN")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "86017")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "U2-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U3-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U4-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U8-5" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))
			(co "OUT^^^" "ElecNet"
				(cv PIN_COUNT "16")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N238" "Net" "$1N238"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N238")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "12289")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C20-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R12-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R15-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "$1N240" "Net" "$1N240"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N240")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "20481")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C20-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R14-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U13-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U13-7" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "$1N241" "Net" "$1N241"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N241")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "24577")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C23-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R15-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U13-5" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "$1N258" "Net" "$1N258"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N258")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "28673")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C21-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R12-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R13-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "OUT" "Net" "OUT"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "OUT")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "94209")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C22-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "P2-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R14-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(o "C20-1,C20-2" "PinPair" "ConnPinPair")
				(o "R12-2,R12-1" "PinPair" "ConnPinPair")
				(o "R14-1,R14-2" "PinPair" "ConnPinPair")
				(o "R15-1,R15-2" "PinPair" "ConnPinPair"))
			(co "U_REF^^^" "ElecNet"
				(cv PIN_COUNT "25")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "(Default)")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "$1N6" "Net" "$1N6"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N6")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "49153")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C9-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R1-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U5-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U11-4" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "$1N32" "Net" "$1N32"
					(cv PIN_COUNT "4")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N32")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "36865")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C2-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C9-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R2-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U5-7" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "$1N37" "Net" "$1N37"
					(cv PIN_COUNT "3")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N37")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "40961")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C1-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R1-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "R2-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "$1N57" "Net" "$1N57"
					(cv PIN_COUNT "2")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "$1N57")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "45057")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C2-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U2-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(co "U_REF" "Net" "U_REF"
					(cv PIN_COUNT "12")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "U_REF")
					(cv PCLASS "(Default)")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "98305")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C1-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C16-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C25-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C26-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C27-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C28-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "P4-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U2-8" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U5-3" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U5-5" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U6-3" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U10-4" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes")))
				(o "C1-1,C1-2" "PinPair" "ConnPinPair")
				(o "C2-1,C2-2" "PinPair" "ConnPinPair")
				(o "C9-1,C9-2" "PinPair" "ConnPinPair")
				(o "R2-2,R2-1" "PinPair" "ConnPinPair"))
			(co "VIN" "ElecNet"
				(cv PIN_COUNT "6")
				(cv ORDER_TYPE "MST")
				(cv POWER_NET "FALSE")
				(cv ECLASS "(All)")
				(cv STUB_LENGTH "300")
				(cv JUMPERS_ALLOWED "Yes")
				(cv PCLASS "supply")
				(cv DELAY_TYPE "Length")
				(cv SIM_DELAY_TYPE "Both")
				(cv ANALOG "FALSE")
				(cv OLDELECNET "FALSE")
				(co "VIN" "Net" "VIN"
					(cv PIN_COUNT "6")
					(cv ORDER_TYPE "MST")
					(cv POWER_NET "FALSE")
					(cv ECLASS "(All)")
					(cv STUB_LENGTH "300")
					(cv JUMPERS_ALLOWED "Yes")
					(cv CDB_NETNAME "VIN")
					(cv PCLASS "supply")
					(cv DELAY_TYPE "Length")
					(cv SIM_DELAY_TYPE "Both")
					(cv CDB_NETNUMBER "102401")
					(cv ANALOG "FALSE")
					(cv OLDELECNET "FALSE")
					(o "C15-2" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "C17-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "P1-1" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U9-6" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U9-7" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))
					(o "U9-8" "Pin"
						(cv POWER_NET "FALSE")
						(cv ECLASS "(All)")
						(cv JUMPERS_ALLOWED "Yes"))))))
	(objectType TOPOTMPL
		(object_count 0))
	(objectType CLASS_CLASS_RULE
		(object_count 2)
		(o "CCR_1"
			(cv C2C_TOCLASS "(All)")
			(cv C2C_RULE "(Default Rule)")
			(cv C2C_FRCLASS "(All)")
			(cv C2C_SCHEME "(Master)"))
		(o "CCR"
			(cv C2C_TOCLASS "(All)")
			(cv C2C_RULE "(Default Rule)")
			(cv C2C_FRCLASS "(All)")
			(cv C2C_SCHEME "(Minimum)")))
	(objectType SCHEME_CLASS_LAYER
		(object_count 22)
		(co "(Master)" "Scheme"
			(co "(Master)/(Default)" "NetClass" "(Default)"
				(cv ROUTE "FALSE")
				(cv VIA_ASSIGN "(default)")
				(o "(Master)/(Default)/SIGNAL_1" "Layer" "SIGNAL_1"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Master)/(Default)/PLANE_2" "Layer" "PLANE_2"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Master)/(Default)/PLANE_3" "Layer" "PLANE_3"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Master)/(Default)/SIGNAL_4" "Layer" "SIGNAL_4"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000")))
			(co "(Master)/supply" "NetClass" "supply"
				(cv ROUTE "FALSE")
				(cv VIA_ASSIGN "(default)")
				(o "(Master)/supply/SIGNAL_1" "Layer" "SIGNAL_1"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Master)/supply/PLANE_2" "Layer" "PLANE_2"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Master)/supply/PLANE_3" "Layer" "PLANE_3"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Master)/supply/SIGNAL_4" "Layer" "SIGNAL_4"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))))
		(co "(Minimum)" "Scheme"
			(co "(Minimum)/(Default)" "NetClass" "(Default)"
				(cv ROUTE "FALSE")
				(cv VIA_ASSIGN "(default)")
				(cv SCLNAME "(Default)")
				(o "(Minimum)/(Default)/SIGNAL_1" "Layer" "SIGNAL_1"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "SIGNAL_1")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Minimum)/(Default)/PLANE_2" "Layer" "PLANE_2"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "PLANE_2")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Minimum)/(Default)/PLANE_3" "Layer" "PLANE_3"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "PLANE_3")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Minimum)/(Default)/SIGNAL_4" "Layer" "SIGNAL_4"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "SIGNAL_4")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000")))
			(co "(Minimum)/supply" "NetClass" "supply"
				(cv ROUTE "FALSE")
				(cv VIA_ASSIGN "(default)")
				(cv SCLNAME "supply")
				(o "(Minimum)/supply/SIGNAL_1" "Layer" "SIGNAL_1"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "SIGNAL_1")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Minimum)/supply/PLANE_2" "Layer" "PLANE_2"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "PLANE_2")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Minimum)/supply/PLANE_3" "Layer" "PLANE_3"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "PLANE_3")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000"))
				(o "(Minimum)/supply/SIGNAL_4" "Layer" "SIGNAL_4"
					(cv MIN_TRACE_WIDTH "7.87401574803150")
					(cv DIFF_SPACING "10")
					(cv ROUTE "true")
					(cv VIA_ASSIGN "(default)")
					(cv EXP_TRACE_WIDTH "7.87401574803150")
					(cv SCLNAME "SIGNAL_4")
					(cv TYP_TRACE_WIDTH "7.87401574803150")
					(cv TYP_IMPEDANCE "0.000000000000")))))
	(objectType LAYER
		(object_count 9)
		(o "DIELECTRIC_1" "Layer" "DIELECTRIC_1"
			(cv CONDUCTOR "None")
			(cv LAYER_TYPE "Insulator")
			(cv HEIGHT "3")
			(cv JOBPREFS_LAYER_NUM "1")
			(cv DIELCONST "1")
			(cv LAYER_DESC "Solder_Mask")
			(cv LAYER_HKP_TECH "LAMINATE")
			(cv JOBPREFS_LAYER_TYPE "DIELECTRIC")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "SIGNAL_1" "Layer" "SIGNAL_1"
			(cv CONDUCTOR "None")
			(cv BULK_RES "0.000000017240")
			(cv LAYER_ENABLED "TRUE")
			(cv LAYER_PAIR "4")
			(cv LAYER_TYPE "Signal")
			(cv HEIGHT "0.7007874015748")
			(cv JOBPREFS_LAYER_NUM "1")
			(cv LAYER_DESC "Microstrip")
			(cv DIELCONST "1.0000")
			(cv LAYER_DIFFPAIR "1")
			(cv DIRECTIONAL_BIAS "HORIZONTAL")
			(cv JOBPREFS_LAYER_TYPE "Signal")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "DIELECTRIC_3" "Layer" "DIELECTRIC_3"
			(cv CONDUCTOR "None")
			(cv LAYER_TYPE "Insulator")
			(cv HEIGHT "20")
			(cv JOBPREFS_LAYER_NUM "3")
			(cv DIELCONST "4.7")
			(cv LAYER_DESC "Core/Pre-preg")
			(cv LAYER_HKP_TECH "LAMINATE")
			(cv JOBPREFS_LAYER_TYPE "DIELECTRIC")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "PLANE_2" "Layer" "PLANE_2"
			(cv CONDUCTOR "None")
			(cv BULK_RES "0.000000017240")
			(cv LAYER_ENABLED "FALSE")
			(cv PNET_UBORDERS "1")
			(cv LAYER_PAIR "3")
			(cv LAYER_TYPE "Signal")
			(cv PLANE_NETS "GND")
			(cv HEIGHT "0.7007874015748")
			(cv JOBPREFS_LAYER_NUM "2")
			(cv PNET_CLEARANCES "300000")
			(cv LAYER_DESC "Plane")
			(cv DIELCONST "1.0000")
			(cv LAYER_DIFFPAIR "2")
			(cv DIRECTIONAL_BIAS "VERTICAL")
			(cv PLANE_TYPE "POSITIVE")
			(cv JOBPREFS_LAYER_TYPE "Plane")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "DIELECTRIC_5" "Layer" "DIELECTRIC_5"
			(cv CONDUCTOR "None")
			(cv LAYER_TYPE "Insulator")
			(cv HEIGHT "20")
			(cv JOBPREFS_LAYER_NUM "5")
			(cv DIELCONST "4.7")
			(cv LAYER_DESC "Core/Pre-preg")
			(cv LAYER_HKP_TECH "LAMINATE")
			(cv JOBPREFS_LAYER_TYPE "DIELECTRIC")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "PLANE_3" "Layer" "PLANE_3"
			(cv CONDUCTOR "None")
			(cv BULK_RES "0.000000017240")
			(cv LAYER_ENABLED "FALSE")
			(cv PNET_UBORDERS "1")
			(cv LAYER_PAIR "2")
			(cv LAYER_TYPE "Signal")
			(cv PLANE_NETS "+5V")
			(cv HEIGHT "0.7007874015748")
			(cv JOBPREFS_LAYER_NUM "3")
			(cv PNET_CLEARANCES "300000")
			(cv LAYER_DESC "Plane")
			(cv DIELCONST "1.0000")
			(cv LAYER_DIFFPAIR "3")
			(cv DIRECTIONAL_BIAS "HORIZONTAL")
			(cv PLANE_TYPE "POSITIVE")
			(cv JOBPREFS_LAYER_TYPE "Plane")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "DIELECTRIC_7" "Layer" "DIELECTRIC_7"
			(cv CONDUCTOR "None")
			(cv LAYER_TYPE "Insulator")
			(cv HEIGHT "20")
			(cv JOBPREFS_LAYER_NUM "7")
			(cv DIELCONST "4.7")
			(cv LAYER_DESC "Core/Pre-preg")
			(cv LAYER_HKP_TECH "LAMINATE")
			(cv JOBPREFS_LAYER_TYPE "DIELECTRIC")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "SIGNAL_4" "Layer" "SIGNAL_4"
			(cv CONDUCTOR "None")
			(cv BULK_RES "0.000000017240")
			(cv LAYER_ENABLED "TRUE")
			(cv LAYER_PAIR "1")
			(cv LAYER_TYPE "Signal")
			(cv HEIGHT "0.7007874015748")
			(cv JOBPREFS_LAYER_NUM "4")
			(cv LAYER_DESC "Microstrip")
			(cv DIELCONST "1.0000")
			(cv LAYER_DIFFPAIR "4")
			(cv DIRECTIONAL_BIAS "VERTICAL")
			(cv JOBPREFS_LAYER_TYPE "Signal")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None"))
		(o "DIELECTRIC_9" "Layer" "DIELECTRIC_9"
			(cv CONDUCTOR "None")
			(cv LAYER_TYPE "Insulator")
			(cv HEIGHT "3")
			(cv JOBPREFS_LAYER_NUM "9")
			(cv DIELCONST "1")
			(cv LAYER_DESC "Solder_Mask")
			(cv LAYER_HKP_TECH "LAMINATE")
			(cv JOBPREFS_LAYER_TYPE "DIELECTRIC")
			(cv TRACE_WIDTH "0")
			(cv EXTRACTED_DIELECTRIC "1.000000")
			(cv LAYER_TECH "None")))
	(objectType PNET
		(object_count 64)
		(co "(Default)" "NetClass" "(Default)"
			(cv ROUTABLE "FALSE")
			(cv PCLASS "(Default)")
			(co "GND" "PowerNet" "GND"
				(cv PIN_COUNT "35")
				(cv SUPPLY_VOLTAGE "0")
				(cv ROUTABLE "FALSE")
				(cv CDB_NETNAME "GND")
				(cv PCLASS "(Default)")
				(cv CDB_NETNUMBER "90113")
				(o "C4-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C5-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C6-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C7-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C8-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C12-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C13-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C14-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C15-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C16-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C17-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C18-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C21-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C22-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C23-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C25-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C26-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C27-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C28-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "P3-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U2-3" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U3-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U3-3" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U4-3" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U5-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U6-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U8-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U9-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U10-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U11-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U11-7" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U12-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U12-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U13-3" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U13-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))))
		(co "supply" "NetClass" "supply"
			(cv ROUTABLE "FALSE")
			(cv PCLASS "(Default)")
			(co "+5V" "PowerNet" "+5V"
				(cv PIN_COUNT "25")
				(cv SUPPLY_VOLTAGE "5")
				(cv ROUTABLE "FALSE")
				(cv CDB_NETNAME "+5V")
				(cv PCLASS "supply")
				(cv CDB_NETNUMBER "81921")
				(o "C4-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C5-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C6-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C7-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C8-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C12-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C13-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C14-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C18-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "C24-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "R9-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "R11-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U2-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U3-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U4-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U4-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U5-8" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U6-5" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U8-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U8-4" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U9-1" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U9-2" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U9-3" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U10-3" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)"))
				(o "U13-8" "Pin"
					(cv ROUTABLE "FALSE")
					(cv PCLASS "(Default)")))))
	(objectType DESIGN
		(object_count 53)
		(co "GENCLEAR" "Design"
			(cv CMH2MH "9.84251968503937")
			(cv TPCENTER2TPCENTER "9.84251968503937")
			(cv PAD2RESISTOR "9.84251968503937")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "9.84251968503937")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "9.84251968503937")
			(cv TRACE2RESISTOR "9.84251968503937")
			(cv PLCOUT2BRDEDGE "9.84251968503937")
			(cv PLCOUT2PLCOB "9.84251968503937")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "9.84251968503937"))
		(co "SCHEMES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(o "(Master)" "Scheme"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(o "(Minimum)" "Scheme"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "NETCLASSES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(co "(Default)" "NetClass"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(co "supply" "NetClass"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "CLEARRULES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(o "(Default Rule)" "ClearRule"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "RULECLASSES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(co "(All)" "Rule"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "LAYERS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(o "SIGNAL_1" "Layer"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(o "PLANE_2" "Layer"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(o "PLANE_3" "Layer"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(o "SIGNAL_4" "Layer"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "VIAS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(o "026VIA" "Via"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(o "VIA" "Via"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "VIASPANS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(co "Through" "ViaSpan"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "VIA")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(o "Through/026VIA" "Via")
				(o "Through/VIA" "Via")))
		(co "TRACES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "PADS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "PARRULEDEFS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "VIAASSIGNS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(o "(Master)/(Default)/Through" "ViaAssign"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE"))
			(o "(Master)/supply/Through" "ViaAssign"
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv P_SIDE "Both")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")))
		(co "CONSTVARS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "DRCS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "PKGTYPERULES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "PHYSBUSSES" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10"))
		(co "PARTTECHS" "Design"
			(cv CMH2MH "10")
			(cv TPCENTER2TPCENTER "10")
			(cv PAD2RESISTOR "10")
			(cv SAMENET_UVIA_OVERLAP "FALSE")
			(cv DEFAULT_VIA "(Default Via)")
			(cv NTV2NTV_PITCH "5")
			(cv P_SIDE "Both")
			(cv NTV2TV_PITCH "5")
			(cv NTVH2TVH_CLEARANCE "5")
			(cv CMH2PC "10")
			(cv SAMENET_UVIA_COINCIDENT "FALSE")
			(cv CMH2NC "10")
			(cv TRACE2RESISTOR "10")
			(cv PLCOUT2BRDEDGE "10")
			(cv PLCOUT2PLCOB "10")
			(cv NTVH2NTVH_CLEARANCE "5")
			(cv PLCOUT2PLCOUT "10")
			(o "ABT" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "AC" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "ACT" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "ALS" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "AS" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "C" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "E10E" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "E10H" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "E10K" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "E100E" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "E100K" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "FAST" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "FCT" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "GTL" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "HC" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "HCT" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "LS" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "S" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10"))
			(o "TTL" "PartTech"
				(cv CMH2MH "10")
				(cv TPCENTER2TPCENTER "10")
				(cv PAD2RESISTOR "10")
				(cv SAMENET_UVIA_OVERLAP "FALSE")
				(cv DEFAULT_VIA "(Default Via)")
				(cv NTV2NTV_PITCH "5")
				(cv P_SIDE "Both")
				(cv NTV2TV_PITCH "5")
				(cv NTVH2TVH_CLEARANCE "5")
				(cv CMH2PC "10")
				(cv SAMENET_UVIA_COINCIDENT "FALSE")
				(cv CMH2NC "10")
				(cv TRACE2RESISTOR "10")
				(cv PLCOUT2BRDEDGE "10")
				(cv PLCOUT2PLCOB "10")
				(cv NTVH2NTVH_CLEARANCE "5")
				(cv PLCOUT2PLCOUT "10")))))
