Mon Oct 13 19:04:08 2008

Note: EnetGenAdapter::Init(F:\MentorGraphics\Angstrem_stend\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Angstrem_stend\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Angstrem_stend\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Angstrem_stend\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Angstrem_stend\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Sun Jul 25 16:47:43 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Warning: Electrical net FB1^^^ has more physical nets than the threshold. One or more of the nets may be a power net. Electrical nets will not be generated.
Note: Net +3.3V has more than 25 pins. It may be an unspecified power net.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Mon Aug 09 17:37:56 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: Net +3.3V has more than 25 pins. It may be an unspecified power net.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Mon Aug 09 17:44:14 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: Net +3.3V has more than 25 pins. It may be an unspecified power net.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Fri Aug 13 12:14:48 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Warning: Electrical net +1.2V^^^ has more physical nets than the threshold. One or more of the nets may be a power net. Electrical nets will not be generated.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Fri Aug 13 12:19:14 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Warning: Electrical net +1.2V^^^ has more physical nets than the threshold. One or more of the nets may be a power net. Electrical nets will not be generated.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Fri Aug 13 13:12:41 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Warning: Electrical net +1.2V^^^ has more physical nets than the threshold. One or more of the nets may be a power net. Electrical nets will not be generated.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
Fri Aug 13 13:42:22 2010

Note: EnetGenAdapter::Init(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PreUpdate(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::Update(F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Warning: Electrical net +1.2V^^^ has more physical nets than the threshold. One or more of the nets may be a power net. Electrical nets will not be generated.
Note: EnetGenAdapter::PostUpdate(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note: EnetGenAdapter::PostSave(1, F:\MentorGraphics\Feedback9\pcb\Work\Layout_Temp\\)
Note:   Data IS modified.
