
                                PLANES PROCESSOR
                                ----------------

                        10:20 AM Monday, August 16, 2010
                Job Name: F:\MentorGraphics\Feedback9\pcb\pcb.pcb




    POSITIVE PLANE LAYER : 1

        Plane Shapes Found On This Layer : 0
        Plane Holes  Found On This Layer : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : YES
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 2mm
            Mounting Hole / Contour Clearance : 2mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : YES
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.4mm
            Default Hatch Distance            : 0.4mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 52
            Total Thru Pads Of This Net       : 10
            Total SMD  Pads Of This Net       : 52

            Plane Created : Layer 1 - Net GND

                Via Pads In This Plane           : 52
                Thru Pads In This Plane          : 10
                SMD Pads In This Plane           : 52
                     
                Pads With 4/4 Tie Connections    : 13
                Pads With 3/4 Tie Connections    : 12
                Pads With 2/4 Tie Connections    : 10
                Pads With 1/4 Tie Connection     : 8
                Pads With 0/4 Tie Connections    : 71

                Total With 0 Tie Connections     : 71
                    Connected To Trace           : 68

                No tieleg connections were due to isolation from plane,
                or the tielegs would have violated clearance requirements,
                or no tielegs were assigned to be created,
                or the pad belongs to a Routed Plane Pin,
                or the pad was a TestPad on top of another connected pad,
                or the pad was contained in a Plane No Connect Area.
                The pads connected to traces are not guaranteed to be
                fully electrically connected.  Connectivity DRC will
                report if this net is not fully connected.

                    Total Pads Not Connected : 3
                        Coordinates (mm) :
                                1) X=46.74       Y=64.43         Pin: U6-4  
                                2) X=76.19       Y=17.78         Pin: P29-1  
                                3) X=76.19       Y=27.94         Pin: P27-1  

                    Pads With 3 Tie Legs : 12
                        Coordinates (mm) :
                                1) X=96.38       Y=78.12         Via  
                                2) X=106.59      Y=70.69         Via  
                                3) X=106.59      Y=62.99         Via  
                                4) X=106.6       Y=78.15         Via  
                                5) X=110.67      Y=62.06         Via  
                                6) X=123.79      Y=61.35         Via  
                                7) X=135.02      Y=45.83         Pin: U29-1  
                                8) X=135.02      Y=68.71         Pin: U28-1  
                                9) X=145.47      Y=54.51         Pin: U26-1  
                               10) X=145.47      Y=77.39         Pin: U25-1  
                               11) X=174.76      Y=49.01         Pin: U30-1  
                               12) X=174.76      Y=71.89         Pin: U27-1  

                    Pads With 2 Tie Legs : 10
                        Coordinates (mm) :
                                1) X=41.78       Y=18.49         Via  
                                2) X=46.74       Y=56.93         Pin: U6-7  
                                3) X=46.74       Y=71.93         Pin: U6-1  
                                4) X=75.73       Y=45.33         Via  
                                5) X=96.37       Y=62.8          Via  
                                6) X=110.67      Y=63.41         Pin: U21-2  
                                7) X=125.27      Y=51.01         Via  
                                8) X=125.27      Y=53.2          Pin: U10-2  
                                9) X=161.3       Y=61.53         Via  
                               10) X=182.48      Y=51.71         Pin: U24-2  

                    Pads With 1 Tie Legs : 8
                        Coordinates (mm) :
                                1) X=70.92       Y=59.83         Via  
                                2) X=72.32       Y=59.83         Via  
                                3) X=75.43       Y=50.08         Via  
                                4) X=110.66      Y=71.23         Pin: U20-2  
                                5) X=110.66      Y=69.79         Via  
                                6) X=110.67      Y=78.58         Pin: U32-2  
                                7) X=110.67      Y=77.15         Via  
                                8) X=182.48      Y=74.59         Pin: U23-2  


    POSITIVE PLANE LAYER : 2

        Plane Shapes Found On This Layer : 0
        Plane Holes  Found On This Layer : 0


        PLANE NET : +3.3V

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : YES
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 0mm
            Mounting Hole / Contour Clearance : 0.25mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.25mm
                Thermal Clearance             : 0.25mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.25mm
                Thermal Clearance             : 0.25mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.25mm
                Thermal Clearance             : 0.25mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : YES
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.25mm
            Default Hatch Distance            : 0.25mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 21
            Total Thru Pads Of This Net       : 1
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 2 - Net +3.3V

                Via Pads In This Plane           : 21
                Thru Pads In This Plane          : 1
                SMD Pads In This Plane           : 0
                     
                Pads With 4/4 Tie Connections    : 18
                Pads With 3/4 Tie Connections    : 3
                Pads With 2/4 Tie Connections    : 1

                    Pads With 3 Tie Legs : 3
                        Coordinates (mm) :
                                1) X=76.19       Y=25.4          Pin: P28-1  
                                2) X=79.64       Y=30.85         Via  
                                3) X=84.27       Y=24.97         Via  

                    Pads With 2 Tie Legs : 1
                        Coordinates (mm) :
                                1) X=108.78      Y=29.4          Via  


    POSITIVE PLANE LAYER : 3

        Plane Shapes Found On This Layer : 2
        Plane Holes  Found On This Layer : 1


        PLANE NET : DGND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 0mm
            Mounting Hole / Contour Clearance : 0.25mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : YES
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.4mm
            Default Hatch Distance            : 0.4mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 41
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net DGND

                Via Pads In This Plane           : 41
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads With 4/4 Tie Connections    : 33
                Pads With 3/4 Tie Connections    : 6
                Pads With 2/4 Tie Connections    : 2

                    Pads With 3 Tie Legs : 6
                        Coordinates (mm) :
                                1) X=79.62       Y=24.97         Via  
                                2) X=87.63       Y=24.42         Via  
                                3) X=87.85       Y=26.58         Via  
                                4) X=89.83       Y=34.33         Via  
                                5) X=92.77       Y=43.79         Via  
                                6) X=94.53       Y=35.29         Via  

                    Pads With 2 Tie Legs : 2
                        Coordinates (mm) :
                                1) X=79.08       Y=32.84         Via  
                                2) X=89.83       Y=16.96         Via  


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : NO
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 0mm
            Mounting Hole / Contour Clearance : 0.25mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : NO
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.4mm
            Default Hatch Distance            : 0.4mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 52
            Total Thru Pads Of This Net       : 10
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net GND

                Via Pads In This Plane           : 52
                Thru Pads In This Plane          : 10
                SMD Pads In This Plane           : 0
                     
                Pads With 4/4 Tie Connections    : 59
                Pads With 3/4 Tie Connections    : 3

                    Pads With 3 Tie Legs : 3
                        Coordinates (mm) :
                                1) X=70.92       Y=59.83         Via  
                                2) X=77.7        Y=38.42         Via  
                                3) X=83.89       Y=53.29         Via  


    POSITIVE PLANE LAYER : 4

        Plane Shapes Found On This Layer : 0
        Plane Holes  Found On This Layer : 0


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : YES
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 2mm
            Mounting Hole / Contour Clearance : 2mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.4mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : YES
            Eliminate Single Tied Areas       : YES
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.4mm
            Default Hatch Distance            : 0.4mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 52
            Total Thru Pads Of This Net       : 10
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 4 - Net GND

                Via Pads In This Plane           : 52
                Thru Pads In This Plane          : 10
                SMD Pads In This Plane           : 0
                     
                Pads With 4/4 Tie Connections    : 24
                Pads With 3/4 Tie Connections    : 6
                Pads With 2/4 Tie Connections    : 5
                Pads With 1/4 Tie Connection     : 5
                Pads With 0/4 Tie Connections    : 22

                Total With 0 Tie Connections     : 22
                    Connected To Trace           : 0

                No tieleg connections were due to isolation from plane,
                or the tielegs would have violated clearance requirements,
                or no tielegs were assigned to be created,
                or the pad belongs to a Routed Plane Pin,
                or the pad was a TestPad on top of another connected pad,
                or the pad was contained in a Plane No Connect Area.

                    Total Pads Not Connected : 22
                        Coordinates (mm) :
                                1) X=44.81       Y=15.51         Via  
                                2) X=46.74       Y=64.43         Pin: U6-4  
                                3) X=53.26       Y=26.46         Via  
                                4) X=67.04       Y=48.9          Via  
                                5) X=72.21       Y=55.46         Via  
                                6) X=72.37       Y=75.79         Via  
                                7) X=75.43       Y=50.08         Via  
                                8) X=75.73       Y=45.33         Via  
                                9) X=75.82       Y=70.08         Via  
                               10) X=76.19       Y=17.78         Pin: P29-1  
                               11) X=76.19       Y=27.94         Pin: P27-1  
                               12) X=77.7        Y=38.42         Via  
                               13) X=77.73       Y=41.31         Via  
                               14) X=83.89       Y=53.29         Via  
                               15) X=84.86       Y=54.13         Via  
                               16) X=96.37       Y=70.46         Via  
                               17) X=96.37       Y=62.8          Via  
                               18) X=96.38       Y=78.12         Via  
                               19) X=100.58      Y=73.38         Via  
                               20) X=103.9       Y=55.53         Via  
                               21) X=106         Y=55.53         Via  
                               22) X=106.59      Y=62.99         Via  

                    Pads With 3 Tie Legs : 6
                        Coordinates (mm) :
                                1) X=34.78       Y=48.53         Pin: P18-1  
                                2) X=37.21       Y=45.84         Via  
                                3) X=68          Y=74.49         Via  
                                4) X=100.42      Y=80.7          Via  
                                5) X=145.47      Y=54.51         Pin: U26-1  
                                6) X=145.47      Y=77.39         Pin: U25-1  

                    Pads With 2 Tie Legs : 5
                        Coordinates (mm) :
                                1) X=46.74       Y=56.93         Pin: U6-7  
                                2) X=46.74       Y=71.93         Pin: U6-1  
                                3) X=70.92       Y=59.83         Via  
                                4) X=72.32       Y=59.83         Via  
                                5) X=99.21       Y=64.61         Via  

                    Pads With 1 Tie Legs : 5
                        Coordinates (mm) :
                                1) X=54.79       Y=23.13         Via  
                                2) X=67.06       Y=34.92         Via  
                                3) X=67.54       Y=54.16         Via  
                                4) X=70.84       Y=64.09         Via  
                                5) X=89.33       Y=55.07         Via  



                        10:20 AM Monday, August 16, 2010