
                                PLANES PROCESSOR
                                ----------------

                         12:47 PM Sunday, July 27, 2008
                 Job Name: F:\MentorGraphics\Arzamas\pcb\pcb.pcb




    POSITIVE PLANE LAYER : 2

        Plane Shapes Found On This Layer : 0
        Plane Holes  Found On This Layer : 4


        PLANE NET : GND

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : YES
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 0.4mm
            Mounting Hole / Contour Clearance : 0.4mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.2mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.2mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.2mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : NO
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.2mm
            Default Hatch Distance            : 0.2mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 11
            Total Thru Pads Of This Net       : 3
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 2 - Net GND

                Via Pads In This Plane           : 11
                Thru Pads In This Plane          : 3
                SMD Pads In This Plane           : 0
                     
                Pads With 4/4 Tie Connections    : 9
                Pads With 3/4 Tie Connections    : 4
                Pads With 1/4 Tie Connection     : 1

                    Pads With 3 Tie Legs : 4
                        Coordinates (mm) :
                                1) X=16.13       Y=6.13          Pin: U11-7  
                                2) X=23.4        Y=7.51          Via  
                                3) X=27.28       Y=10.56         Via  
                                4) X=30.04       Y=16.6          Via  

                    Pads With 1 Tie Legs : 1
                        Coordinates (mm) :
                                1) X=28.89       Y=16.68         Via  


    POSITIVE PLANE LAYER : 3

        Plane Shapes Found On This Layer : 0
        Plane Holes  Found On This Layer : 3


        PLANE NET : +5V

            Total Plane Shapes For This Net   : 1
            Use Route Border As Plane Shape   : YES
            Create Actual Plane Shapes        : NO
            Regenerate APS Connections Only   : NO
            Generate Plane Data               : YES
            Plane To Plane Clearance          : 0.2mm
            Plane To Other Metal Clearance    : 0.4mm
            Mounting Hole / Contour Clearance : 0.4mm
            Minimum Plane Gap Distance        : NA
            Use TieLeg Bridges If Needed      : NO
            Use Padstack Thermal Definition   : YES
            Default Via Tie Properties
                Tie Leg Width                 : 0.2mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default Thru Tie Properties
                Tie Leg Width                 : 0.2mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Default SMD Tie Properties
                Tie Leg Width                 : 0.2mm
                Thermal Clearance             : 0.2mm
                Number Tie Legs               : FOUR
                Tie Orientation               : PREFER 0
            Eliminate Untied Areas            : NO
            Eliminate Single Tied Areas       : NO
            Orthogonal Data Only              : NO
            Discard Areas By Dimension        : NO
            Default Hatch Width               : 0.2mm
            Default Hatch Distance            : 0.2mm
            Default Hatch Pattern             : (|) Vertical
            Default Metal Percentage          : 100.00

            Total Via  Pads Of This Net       : 9
            Total Thru Pads Of This Net       : 0
            Total SMD  Pads Of This Net       : 0

            Plane Created : Layer 3 - Net +5V

                Via Pads In This Plane           : 9
                Thru Pads In This Plane          : 0
                SMD Pads In This Plane           : 0
                     
                Pads With 4/4 Tie Connections    : 5
                Pads With 3/4 Tie Connections    : 3
                Pads With 2/4 Tie Connections    : 1

                    Pads With 3 Tie Legs : 3
                        Coordinates (mm) :
                                1) X=19.77       Y=6.88          Via  
                                2) X=24.87       Y=6.66          Via  
                                3) X=28.8        Y=15.58         Via  

                    Pads With 2 Tie Legs : 1
                        Coordinates (mm) :
                                1) X=29.04       Y=17.78         Via  



                        12:47 PM Sunday, July 27, 2008